# Contents

|  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- | --- |
| |  |  |  | | --- | --- | --- | | ID | Part | QTY | | 1 | LipSync Joystick | 1 | | 2 | LipSync Hub | 1 | | 3 | LipSync Interface Cable | 1 | | 4 | LipSync Hub Stand | 1 | | 5 | LipSync Mouthpieces | 5 | | 6 | USB-C – USB-A Cable | 1 | |  |

# Setup Instructions

1. Mount the LipSync Joystick.
2. Mount the Hub on the Hub Stand.
3. Connect the Joystick to the Hub using the Interface Cable.
4. Attach a mouthpiece to the Joystick.
5. Connect the Hub to the Host Device using a USB Cable.

# Additional Documentation

|  |  |
| --- | --- |
| LipSync Quickstart Guide PDF QR Code[Quickstart Guide](https://github.com/makersmakingchange/LipSync/blob/main/Documentation/LipSync_Quickstart_Guide.pdf) | **LipSync User Guide PDF QR Code**[User Guide](https://github.com/makersmakingchange/LipSync/blob/main/Documentation/LipSync_User_Guide.pdf) |